#txt
# -----------------------------------------------------------------------------
# This file "lddefault.txt" is provided as a convenience for upgrading the
# Cisco 7905G IP Phone with minimal effort.  
#
# If changes are made to this file, you must run 
#
#         cfgfmt -tsip_ptag.dat lddefault.txt lddefault.cfg
#
# again to create a new profile and place it in the TFTP directory.
#
# If you plan to upgrade just one phone, you can copy lddefault.cfg to
# ld<MAC>, where <MAC> is the MAC address of the target phone, such
# as ld001122334455.
#
# The phone will try to download ld<mac> first, then lddefault.cfg
# if corresponding ld<MAC> is not found on the TFTP server.
# -----------------------------------------------------------------------------
#
#
#example: bmp2logo.exe 10 newlogo.bmp newlogo.logo
#
#and then in your config txt file you have to add:
#upgradelogo:$imageid,0,$logo_filename
#
#so in this case it would be:
#upgradelogo:22,0,pero.logo 
#
#
#
upgradecode:3,0x501,0x0400,0x0100,0.0.0.0,69,0x060111a,CP7905080000SIP060111B.zup
upgradelogo:9,0,3CX.logo  





dhcp:1
SIPRegOn:1
UID:2356
TimeZone:1
NTPIP:161.53.123.5
UseTftp:1
ShortName:Cisco 7905

TimeFormat:H:i
DateFormat:d-M-Y

# Set the GUI/Web config password to 2356; the password must NOT be 0 
# (disabled) if configuring via the phone's web interface is desired.
UIPassword:2356
